**Küberit focuses on convenience and safety**

*10 January 2020; Küberit, Lüdenscheid. –* **Small changes sometimes have big effects: Küberit has optimised its profiles in order to make installation easier and to extend the range of possible applications. At Domotex in January, the profile specialist will once again demonstrate its excellence in making its aluminium profiles and profile systems technically more and more convenient, sustainable and flexible, with the aid of smart modifications: new profile heights, new lengths and a new installation process.**

Küberit has added new technical features to its well-known Motion-Star expansion joint profile series and its silicon and double-K profiles. "With our innovations, we consistently focus on further development and always try to think one step ahead. We optimise our profiles on the basis of feedback from the market and experiences gleaned during practical application. Sometimes these are only small changes, but they add genuine value when it comes to installation: The technical innovations always make the installer's work easier and at the same time expand the range of possible applications on the construction site," says Lars Maier, Sales Manager Germany.

**Self-adhesive Motion-Star**

With the new expansion joint profile 316 for floor coverings up to 2.2 mm, Küberit offers a further version of the already well-known Motion Star profile series. The new self-adhesive variants make installation easier. The profiles are simply stuck and sealed at the marked starting position on the floor. This kind of installation has several advantages: It is a safe installation aid, very time-saving and no further accessories are needed - this makes processing errors virtually impossible.

**Less waste, faster installation**

Küberit has now developed a 3-metre version of the most important profile heights of the silicone and the double-K profiles. For the installer this means: less waste, fewer joints, faster assembly, fewer sources of error. The new 2.5-metre expansion joint profile 300 S with silicone for coverings up to 2.5 mm is faster and more convenient to install for the same reasons.

**Photo caption:**

**A focus on convenient installation:** The new Motion-Star self-adhesive profile systems for coverings up to 2.2 mm in height ensure significantly safer and faster installation. The new length of 3 metres for the most important profile heights of the silicone and double-K profiles also ensures less waste.

***All photos:*** Küberit

Reprint permitted: 2,345 characters (incl. spaces)

**About Küberit Profile Systems GmbH & Co. KG**

As a globally successful manufacturer of floor and stair profiles, the name Küberit has stood for quality and progress for 157 years. Customer satisfaction, perfection, innovation and the preservation of our tradition are integral parts of our corporate philosophy. Constant investments in the latest technologies and certifications guarantee the continuously high quality of our products and services. Küberit is one of the first profile manufacturers to be certified according to DIN EN ISO 9001:2015 and has been so since September 2016.